Par Statistics
Total Non-vccgnd Signals=4077
Total Non-vccgnd Design Pins=18349
Total Non-vccgnd Conns=18349
Total Non-vccgnd Timing Constrained Conns=15309
Phase 1 CPU=10.8 sec
Phase 2 CPU=14.2 sec
Phase 3 CPU=23.6 sec
Phase 4 CPU=27.9 sec
Phase 5 CPU=36.7 sec
Phase 6 CPU=38.3 sec
Phase 7 CPU=38.3 sec
Phase 8 CPU=38.3 sec
Phase 9 CPU=39.2 sec
Phase 10 CPU=40.3 sec
AvgWirelenPerPin Fanout 1=3.0
AvgWirelenPerPin Fanout 2=2.5
AvgWirelenPerPin Fanout 3=3.3
AvgWirelenPerPin Fanout 4=4.3
AvgWirelenPerPin Fanout 10=2.7
AvgWirelenPerPin Fanout 50=4.0
AvgWirelenPerPin Fanout 100=4.8
AvgWirelenPerPin Fanout 500=7.6
AvgWirelenPerPin Fanout 5000=4.8
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
IRR Gamma=1.5038