### Device Usage Page (usage_statistics_webtalk.html)

This HTML page displays the device usage statistics that will be sent to Xilinx.

Software Version and Target Device
Product Version: | ISE:12.3 (ISE) - M.70d | Target Family: | Spartan6
OS Platform: | NT64 | Target Device: | xc6slx45
Project ID (random number) | 67a15295ee104f8eb91a0ab5f5167ee8.E0B60106E9D849C5917F344B8FD41FA5.2 | Target Package: | csg324
Registration ID | No user information available. | Target Speed: | -3
Date Generated | 2012-12-19T13:42:44 | Tool Flow | ISE

User Environment
OS Name | Microsoft | OS Release | Service Pack 1 (build 7601)
CPU Name | Intel(R) Core(TM) i7-2670QM CPU @ 2.20GHz | CPU Speed | 2195 MHz
OS Name | Microsoft | OS Release | Service Pack 1 (build 7601)
CPU Name | Intel(R) Core(TM) i7-2670QM CPU @ 2.20GHz | CPU Speed | 2195 MHz

Device Usage Statistics
Macro Statistics | Miscellaneous Statistics | Net Statistics | Site Usage
Adders/Subtractors=333 16-bit adder=64 17-bit adder=3 2-bit adder=16 31-bit adder=16 4-bit adder=27 4-bit addsub=16 5-bit adder=8 6-bit adder=16 6-bit subtractor=16 8-bit adder=70 8-bit addsub=8 8-bit subtractor=51 9-bit adder=14 9-bit subtractor=8 Comparators=150 31-bit comparator equal=8 31-bit comparator greater=8 4-bit comparator greater=32 4-bit comparator lessequal=8 8-bit comparator greater=72 8-bit comparator lessequal=6 9-bit comparator greater=16 Counters=83 4-bit up counter=19 6-bit up counter=32 8-bit up counter=32 FSMs=116 Multiplexers=9486 1-bit 2-to-1 multiplexer=7695 1-bit 3-to-1 multiplexer=8 1-bit 4-to-1 multiplexer=32 1-bit 5-to-1 multiplexer=8 1-bit 6-to-1 multiplexer=8 16-bit 2-to-1 multiplexer=215 16-bit 3-to-1 multiplexer=3 17-bit 2-to-1 multiplexer=45 2-bit 2-to-1 multiplexer=232 4-bit 2-to-1 multiplexer=576 4-bit 3-to-1 multiplexer=16 6-bit 2-to-1 multiplexer=48 8-bit 2-to-1 multiplexer=562 8-bit 3-to-1 multiplexer=3 8-bit 4-to-1 multiplexer=11 9-bit 2-to-1 multiplexer=21 9-bit 4-to-1 multiplexer=3 Multipliers=3 8x4-bit multiplier=3 RAMs=75 16x1-bit single-port distributed Read Only RAM=24 256x8-bit dual-port distributed RAM=16 32x8-bit single-port distributed Read Only RAM=8 64x8-bit dual-port distributed RAM=16 8192x8-bit dual-port distributed RAM=3 8x1-bit single-port distributed Read Only RAM=8 Registers=3764 Flip-Flops=3764 | MiscellaneousStatistics AGG_BONDED_IO=10 AGG_IO=10 AGG_SLICE=4676 NUM_BONDED_IOB=10 NUM_BSFULL=4079 NUM_BSLUTONLY=12226 NUM_BSREGONLY=260 NUM_BSUSED=16565 NUM_BUFG=4 NUM_DPRAM_O6ONLY=5528 NUM_LOGIC_O5ANDO6=1927 NUM_LOGIC_O5ONLY=569 NUM_LOGIC_O6ONLY=8169 NUM_LUT_RT_DRIVES_CARRY4=72 NUM_LUT_RT_EXO6=72 NUM_LUT_RT_O5=10 NUM_LUT_RT_O6=569 NUM_SLICEL=476 NUM_SLICEM=1392 NUM_SLICEX=2808 NUM_SLICE_CARRY4=194 NUM_SLICE_CONTROLSET=1154 NUM_SLICE_CYINIT=18883 NUM_SLICE_F7MUX=290 NUM_SLICE_FF=3798 NUM_SLICE_LATCH=782 NUM_SLICE_UNUSEDCTRL=1234 NUM_SPRAM_O6ONLY=40 NUM_UNUSABLE_FF_BELS=4356 | NetStatistics NumNets_Active=18220 NumNets_Gnd=1 NumNets_Vcc=1 NumNodesOfType_Active_BOUNCEACROSS=1416 NumNodesOfType_Active_BOUNCEIN=3581 NumNodesOfType_Active_BUFGOUT=4 NumNodesOfType_Active_BUFHINP2OUT=22 NumNodesOfType_Active_CLKPIN=3442 NumNodesOfType_Active_CLKPINFEED=34 NumNodesOfType_Active_CNTRLPIN=3147 NumNodesOfType_Active_DOUBLE=52282 NumNodesOfType_Active_GENERIC=7 NumNodesOfType_Active_GLOBAL=463 NumNodesOfType_Active_INPUT=126 NumNodesOfType_Active_IOBIN2OUT=5 NumNodesOfType_Active_IOBOUTPUT=5 NumNodesOfType_Active_LUTINPUT=87001 NumNodesOfType_Active_OUTBOUND=17369 NumNodesOfType_Active_OUTPUT=18722 NumNodesOfType_Active_PADINPUT=4 NumNodesOfType_Active_PADOUTPUT=2 NumNodesOfType_Active_PINBOUNCE=16851 NumNodesOfType_Active_PINFEED=91097 NumNodesOfType_Active_QUAD=30841 NumNodesOfType_Active_REGINPUT=5423 NumNodesOfType_Active_SINGLE=57703 NumNodesOfType_Vcc_HVCCOUT=1333 NumNodesOfType_Vcc_KVCCOUT=25 NumNodesOfType_Vcc_LUTINPUT=2626 NumNodesOfType_Vcc_PINBOUNCE=21 NumNodesOfType_Vcc_PINFEED=2626 NumNodesOfType_Vcc_REGINPUT=21 SiteStatistics BUFG-BUFGMUX=4 IOB-IOBM=5 IOB-IOBS=5 SLICEL-SLICEM=109 SLICEX-SLICEL=752 SLICEX-SLICEM=35 | SiteSummary BUFG=4 BUFG_BUFG=4 CARRY4=194 FF_SR=354 HARD0=72 IOB=10 IOB_IMUX=2 IOB_INBUF=2 IOB_OUTBUF=8 LUT5=2506 LUT6=10737 LUT_OR_MEM6=5568 PAD=10 REG_SR=4226 SELMUX2_1=290 SLICEL=476 SLICEM=1392 SLICEX=2808

Configuration Data
FF_SR CK=[CK:354] [CK_INV:0] SRINIT=[SRINIT0:354] SYNC_ATTR=[ASYNC:194] [SYNC:160] IOB_OUTBUF DRIVEATTRBOX=[12:8] SLEW=[SLOW:8] SUSPEND=[3STATE:8] | LUT_OR_MEM6 CLK=[CLK:5568] [CLK_INV:0] LUT_OR_MEM=[RAM:5568] RAMMODE=[SPRAM64:40] [DPRAM64:5528] REG_SR CK=[CK:3452] [CK_INV:774] LATCH_OR_FF=[FF:3444] [LATCH:782] SRINIT=[SRINIT0:4179] [SRINIT1:47] SYNC_ATTR=[ASYNC:3051] [SYNC:1175] | SLICEL CLK=[CLK:263] [CLK_INV:88] SLICEM CLK=[CLK:1392] [CLK_INV:0] SLICEX CLK=[CLK:1412] [CLK_INV:287]

Pin Data
BUFG I0=4 O=4 BUFG_BUFG I0=4 O=4 CARRY4 CIN=122 CO3=122 CYINIT=72 DI0=176 DI1=176 DI2=173 DI3=122 O0=194 O1=176 O2=176 O3=173 S0=194 S1=176 S2=176 S3=173 FF_SR CE=242 CK=354 D=354 Q=354 SR=181 HARD0 0=72 IOB I=2 O=8 PAD=10 IOB_IMUX I=2 OUT=2 IOB_INBUF OUT=2 PAD=2 IOB_OUTBUF IN=8 OUT=8 LUT5 A1=1265 A2=1419 A3=1647 A4=1534 A5=1530 O5=2506 LUT6 A1=6169 A2=8230 A3=9268 A4=10105 A5=10349 A6=10671 O6=10737 LUT_OR_MEM6 A1=5568 A2=5568 A3=5568 A4=5568 A5=5568 A6=5568 CLK=5568 DI1=5568 O6=4640 WA1=5568 WA2=5568 WA3=5568 WA4=5568 WA5=5568 WA6=5568 WE=5568 | PAD PAD=10 REG_SR CE=2593 CK=4226 D=4226 Q=4226 SR=1288 SELMUX2_1 0=290 1=290 OUT=290 S0=290 SLICEL A=194 A1=195 A2=242 A3=247 A4=329 A5=353 A6=443 AMUX=152 AQ=186 AX=51 B=259 B1=222 B2=256 B3=277 B4=356 B5=382 B6=457 BMUX=184 BQ=134 BX=23 C=7 C1=145 C2=246 C3=252 C4=359 C5=391 C6=470 CE=207 CIN=122 CLK=351 CMUX=271 COUT=122 CQ=223 CX=308 D=8 D1=184 D2=250 D3=284 D4=372 D5=376 D6=439 DMUX=102 DQ=146 DX=73 SR=108 | SLICEM A=1392 A1=1392 A2=1392 A3=1392 A4=1392 A5=1392 A6=1392 AQ=2 AX=1379 B=1392 B1=1392 B2=1392 B3=1392 B4=1392 B5=1392 B6=1392 BQ=1 BX=919 C=928 C1=1392 C2=1392 C3=1392 C4=1392 C5=1392 C6=1392 CE=1392 CLK=1392 CX=1377 D=928 D1=1392 D2=1392 D3=1392 D4=1392 D5=1392 D6=1392 DX=1392 SR=3 SLICEX A=1606 A1=1779 A2=2211 A3=2353 A4=2446 A5=2440 A6=2442 AMUX=411 AQ=1181 AX=296 B=1675 B1=1629 B2=2000 B3=2181 B4=2263 B5=2310 B6=2317 BMUX=543 BQ=871 BX=190 C=1522 C1=1464 C2=1867 C3=2075 C4=2139 C5=2174 C6=2176 CE=920 CLK=1699 CMUX=453 CQ=872 CX=192 D=1511 D1=1375 D2=1702 D3=1845 D4=1894 D5=1923 D6=1927 DMUX=318 DQ=610 DX=177 SR=532 |

Tool Usage
Command Line History xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx100-fgg484-3 <ise_file> <fname>.ngd xst -intstyle ise -ifn <ise_file> ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx100-fgg484-3 <ise_file> <fname>.ngd xst -intstyle ise -ifn <ise_file> ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx100-fgg484-3 <ise_file> <fname>.ngd xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx100-fgg484-3 <ise_file> <fname>.ngd xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx4-tqg144-3 <ise_file> <fname>.ngd xst -intstyle ise -ifn <ise_file> ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx4-tqg144-3 <ise_file> <fname>.ngd map -intstyle ise -p xc6slx4-tqg144-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf xst -intstyle ise -ifn <ise_file> ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx45-csg324-3 <ise_file> <fname>.ngd map -intstyle ise -p xc6slx45-csg324-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx45-csg324-3 <ise_file> <fname>.ngd map -intstyle ise -p xc6slx45-csg324-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf trce -intstyle ise -v 3 -s 3 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf bitgen -intstyle ise -f <fname>.ut <fname>.ncd xst -intstyle ise -ifn <ise_file> xst -intstyle ise -ifn <ise_file> ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx45-csg324-3 <ise_file> <fname>.ngd map -intstyle ise -p xc6slx45-csg324-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf xst -intstyle ise -ifn <ise_file> ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx45-csg324-3 <ise_file> <fname>.ngd map -intstyle ise -p xc6slx45-csg324-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf trce -intstyle ise -v 3 -s 3 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx45-csg324-3 <ise_file> <fname>.ngd map -intstyle ise -p xc6slx45-csg324-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf trce -intstyle ise -v 3 -s 3 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf xst -intstyle ise -ifn <ise_file> ngdbuild -intstyle ise -dd _ngo -nt timestamp -uc <fname>.ucf -p xc6slx45-csg324-3 <ise_file> <fname>.ngd map -intstyle ise -p xc6slx45-csg324-3 -w -logic_opt off -ol high -t 1 -xt 0 -register_duplication off -global_opt off -mt off -ir off -pr off -lc off -power off -o <fname>.ncd <fname>.ngd <fname>.pcf par -w -intstyle ise -ol high -mt off <fname>.ncd <fname>.ncd <fname>.pcf trce -intstyle ise -v 3 -s 3 -n 3 -fastpaths -xml <fname>.twx <fname>.ncd -o <fname>.twr <fname>.pcf -ucf <fname>.ucf bitgen -intstyle ise -f <fname>.ut <fname>.ncd fuse

Software Quality
Run Statistics
_impact | 3 | 3 | 0 | 0 | 0 | 0 | 0
bitgen | 7 | 7 | 0 | 0 | 0 | 0 | 0
compxlib | 4 | 4 | 0 | 0 | 0 | 0 | 0
cxlgui | 1 | 1 | 0 | 0 | 0 | 0 | 0
map | 75 | 58 | 0 | 0 | 0 | 0 | 0
netgen | 10 | 10 | 0 | 0 | 0 | 0 | 0
ngc2edif | 6 | 6 | 0 | 0 | 0 | 0 | 0
ngcbuild | 5 | 5 | 0 | 0 | 0 | 0 | 0
ngdbuild | 75 | 75 | 0 | 0 | 0 | 0 | 0
par | 59 | 56 | 3 | 0 | 0 | 0 | 0
partgen | 22 | 21 | 0 | 0 | 0 | 0 | 0
platgen | 5 | 1 | 0 | 0 | 0 | 0 | 0
trce | 61 | 61 | 0 | 0 | 0 | 0 | 0
xbash | 1 | 1 | 0 | 0 | 0 | 0 | 0
xps | 9 | 9 | 0 | 0 | 0 | 0 | 0
xst | 453 | 425 | 0 | 0 | 0 | 0 | 0

Help Statistics
Search words with results
Xst ( 1 ) | Xst error ( 1 )
attribute ( 1 ) | clock ( 1 )
clock input ( 1 )
Unsuccessful Search words
unsupported clock ( 1 )
Help files
/doc/usenglish/isehelp/cgn_c_df_vhdl_create_test_bench.htm ( 1 ) | /doc/usenglish/isehelp/cgn_c_df_vhdl_flow.htm ( 1 )
/doc/usenglish/isehelp/cgn_db_advanced_options.htm ( 1 ) | /doc/usenglish/isehelp/devref.pdf ( 1 )
/doc/usenglish/isehelp/dsm_p_showing_new_messages.htm ( 1 ) | /doc/usenglish/isehelp/dsm_p_using_message_filters_commandline.htm ( 1 )
/doc/usenglish/isehelp/ise_c_lt_adding_code_using_language_templates.htm ( 1 ) | /doc/usenglish/isehelp/ise_c_report_clock_resource_utilization.htm ( 1 )
/doc/usenglish/isehelp/ise_c_understanding_design_parser.htm ( 1 ) | /doc/usenglish/isehelp/ise_c_working_with_source_control.htm ( 1 )
/doc/usenglish/isehelp/ise_c_working_with_vhdl_libraries.htm ( 1 ) | /doc/usenglish/isehelp/ise_n_devref_guide.htm ( 1 )
/doc/usenglish/isehelp/ise_p_generate_fpga_programming_file.htm ( 1 ) | /doc/usenglish/isehelp/ise_r_properties_conversion_ise10_ise11.htm ( 1 )
/doc/usenglish/isehelp/ise_r_source_types.htm ( 1 ) | /doc/usenglish/isehelp/ite_c_overview.htm ( 2 )
/doc/usenglish/isehelp/ite_r_vhdl_reserved_words.htm ( 1 ) | /doc/usenglish/isehelp/pce_c_clock_to_pad_top.htm ( 1 )
/doc/usenglish/isehelp/pim_p_addingfiles_promdevices.htm ( 1 ) | /doc/usenglish/isehelp/pim_p_addingfiles_systemacecf.htm ( 1 )
/doc/usenglish/isehelp/pim_r_supported_spi_bpi_proms.htm ( 1 ) | /doc/usenglish/isehelp/pn_db_design_view_properties.htm ( 1 )
/doc/usenglish/isehelp/pn_db_nsw_select_source_type.htm ( 1 ) | /doc/usenglish/isehelp/pp_db_configuration_options.htm ( 1 )
/doc/usenglish/isehelp/pp_p_process_configure_target_device.htm ( 1 ) | /doc/usenglish/isehelp/pp_p_process_io_pin_planning_post_syn.htm ( 1 )
/doc/usenglish/isehelp/pta_db_analyze_against_user_specified_paths_button.htm ( 1 ) | /doc/usenglish/isehelp/pta_db_ttc-clock-io-page.htm ( 1 )
/doc/usenglish/isehelp/sse_c_attr_traits.htm ( 1 ) | /doc/usenglish/isehelp/sse_c_intro_to_attrs.htm ( 1 )
/doc/usenglish/isehelp/sse_p_adding_attr.htm ( 1 ) | /doc/usenglish/isehelp/sse_p_adding_xilinx_constraints.htm ( 1 )
/doc/usenglish/isehelp/xpa_c_clock_domain_view.htm ( 1 )

Project Statistics
PROP_Enable_Message_Filtering=false | PROP_FitterReportFormat=HTML
PROP_ISimsUseCustomWaveConfigFile_behav=true | PROP_LastAppliedGoal=Balanced
PROP_LastAppliedStrategy=Xilinx Default (unlocked) | PROP_ManualCompileOrderImp=false
PROP_PropSpecInProjFile=Store all values | PROP_SelectedInstanceHierarchicalPath=/MultiMPITest
PROP_Simulator=ISim (VHDL/Verilog) | PROP_SynthTopFile=changed
PROP_Top_Level_Module_Type=HDL | PROP_UseSmartGuide=false
PROP_UserConstraintEditorPreference=Text Editor | PROP_intProjectCreationTimestamp=2011-07-02T09:03:34
PROP_intWbtProjectID=E0B60106E9D849C5917F344B8FD41FA5 | PROP_intWbtProjectIteration=2
PROP_intWorkingDirLocWRTProjDir=Same | PROP_intWorkingDirUsed=No
PROP_lockPinsUcfFile=changed | PROP_selectedSimRootSourceNode_behav=work.MultiMPITest
PROP_selectedSimRootSourceNode_translate=NocLib.stimuli45 | PROP_xilxSynthKeepHierarchy=Soft
PROPEXT_mapTimingMode_spartan6=Non Timing Driven | PROP_AutoTop=false
PROP_DevFamily=Spartan6 | PROP_ISimsUseCustomWaveConfigFilename_behav=changed
PROP_CompxlibSimPath=changed | PROP_DevDevice=xc6slx45
PROP_DevFamilyPMName=spartan6 | PROP_ISimSimulationRunTime_behav_tb=200 ns
PROP_DevPackage=csg324 | PROP_Synthesis_Tool=XST (VHDL/Verilog)
PROP_DevSpeed=-3 | PROP_PreferredLanguage=VHDL
FILE_UCF=2 | FILE_VHDL=58

Unisim Statistics
NGDBUILD_PRE_UNISIM_SUMMARY
NGDBUILD_NUM_BUFG=3 | NGDBUILD_NUM_BUFGP=1 | NGDBUILD_NUM_FD=293 | NGDBUILD_NUM_FDC=120
NGDBUILD_NUM_FDE=2044 | NGDBUILD_NUM_FDP=16 | NGDBUILD_NUM_FDR=520 | NGDBUILD_NUM_FDRE=791
NGDBUILD_NUM_FDS=24 | NGDBUILD_NUM_GND=71 | NGDBUILD_NUM_IBUF=1 | NGDBUILD_NUM_INV=142
NGDBUILD_NUM_LD=774 | NGDBUILD_NUM_LDC=8 | NGDBUILD_NUM_LUT1=641 | NGDBUILD_NUM_LUT2=787
NGDBUILD_NUM_LUT3=1206 | NGDBUILD_NUM_LUT4=1461 | NGDBUILD_NUM_LUT5=2884 | NGDBUILD_NUM_LUT6=5609
NGDBUILD_NUM_MUXCY=647 | NGDBUILD_NUM_MUXF7=290 | NGDBUILD_NUM_OBUF=8 | NGDBUILD_NUM_RAM64M=928
NGDBUILD_NUM_RAM64X1D=928 | NGDBUILD_NUM_VCC=49 | NGDBUILD_NUM_XORCY=719
NGDBUILD_POST_UNISIM_SUMMARY
NGDBUILD_NUM_BUFG=4 | NGDBUILD_NUM_FD=293 | NGDBUILD_NUM_FDC=120 | NGDBUILD_NUM_FDE=2044
NGDBUILD_NUM_FDP=16 | NGDBUILD_NUM_FDR=520 | NGDBUILD_NUM_FDRE=791 | NGDBUILD_NUM_FDS=24
NGDBUILD_NUM_GND=71 | NGDBUILD_NUM_IBUF=1 | NGDBUILD_NUM_IBUFG=1 | NGDBUILD_NUM_INV=142
NGDBUILD_NUM_LD=774 | NGDBUILD_NUM_LDC=8 | NGDBUILD_NUM_LUT1=641 | NGDBUILD_NUM_LUT2=787
NGDBUILD_NUM_LUT3=1206 | NGDBUILD_NUM_LUT4=1461 | NGDBUILD_NUM_LUT5=2884 | NGDBUILD_NUM_LUT6=5609
NGDBUILD_NUM_MUXCY=647 | NGDBUILD_NUM_MUXF7=290 | NGDBUILD_NUM_OBUF=8 | NGDBUILD_NUM_RAM64M=928
NGDBUILD_NUM_TS_TIMESPEC=1 | NGDBUILD_NUM_VCC=49 | NGDBUILD_NUM_XORCY=719

ISim Statistics
Xilinx HDL Libraries Used=
Fuse Resource Usage=1621 ms, 43752 KB
Total Signals=2855
Total Nets=1092412
Total Blocks=167
Total Processes=810
Total Simulation Time=22200 ns
Simulation Resource Usage=3.29162 sec, 1899794 KB
Simulation Mode=gui
Hardware CoSim=0