Par Statistics
Total Non-vccgnd Signals=17333
Total Non-vccgnd Design Pins=99193
Total Non-vccgnd Conns=99193
Total Non-vccgnd Timing Constrained Conns=88443
Phase 1 CPU=20.7 sec
Phase 2 CPU=23.9 sec
Phase 3 CPU=104.2 sec
Phase 4 CPU=194.7 sec
Phase 5 CPU=290.6 sec
Phase 6 CPU=367.8 sec
Phase 7 CPU=421.3 sec
Phase 8 CPU=421.3 sec
Phase 9 CPU=421.3 sec
Phase 10 CPU=430.2 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=2.5
AvgWirelenPerPin Fanout 3=4.3
AvgWirelenPerPin Fanout 4=4.0
AvgWirelenPerPin Fanout 10=3.1
AvgWirelenPerPin Fanout 50=2.0
AvgWirelenPerPin Fanout 100=5.4
AvgWirelenPerPin Fanout 500=5.1
AvgWirelenPerPin Fanout 5000=3.7
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
IRR Gamma=24.5487