Par Statistics
Total Non-vccgnd Signals=12127
Total Non-vccgnd Design Pins=75043
Total Non-vccgnd Conns=75043
Total Non-vccgnd Timing Constrained Conns=66414
Phase 1 CPU=17.6 sec
Phase 2 CPU=20.7 sec
Phase 3 CPU=96.9 sec
Phase 4 CPU=214.1 sec
Phase 5 CPU=331.6 sec
Phase 6 CPU=541.2 sec
Phase 7 CPU=639.5 sec
Phase 8 CPU=639.5 sec
Phase 9 CPU=639.5 sec
Phase 10 CPU=646.6 sec
AvgWirelenPerPin Fanout 1=4.0
AvgWirelenPerPin Fanout 2=3.0
AvgWirelenPerPin Fanout 3=6.3
AvgWirelenPerPin Fanout 4=5.3
AvgWirelenPerPin Fanout 10=3.4
AvgWirelenPerPin Fanout 50=2.7
AvgWirelenPerPin Fanout 100=6.5
AvgWirelenPerPin Fanout 500=5.0
AvgWirelenPerPin Fanout 5000=3.4
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
IRR Gamma=11.2011