Par Statistics
Total Non-vccgnd Signals=24642
Total Non-vccgnd Design Pins=150592
Total Non-vccgnd Conns=150592
Total Non-vccgnd Timing Constrained Conns=130230
Phase 1 CPU=31.9 sec
Phase 2 CPU=36.2 sec
Phase 3 CPU=186.8 sec
Phase 4 CPU=456.3 sec
Phase 5 CPU=762.5 sec
Phase 6 CPU=1529.4 sec
Phase 7 CPU=1638.8 sec
Phase 8 CPU=1638.8 sec
Phase 9 CPU=1638.8 sec
Phase 10 CPU=1653.8 sec
AvgWirelenPerPin Fanout 1=5.0
AvgWirelenPerPin Fanout 2=3.0
AvgWirelenPerPin Fanout 3=6.0
AvgWirelenPerPin Fanout 4=4.8
AvgWirelenPerPin Fanout 10=3.5
AvgWirelenPerPin Fanout 50=2.7
AvgWirelenPerPin Fanout 100=6.7
AvgWirelenPerPin Fanout 500=6.4
AvgWirelenPerPin Fanout 5000=3.8
AvgWirelenPerPin Fanout 20000=0.0
AvgWirelenPerPin Fanout 50000=0.0
IRR Gamma=17.4104