# $NetBSD: INSTALL_MALTA,v 1.1.2.2 2011/05/26 19:22:46 matt Exp $

include		"arch/evbmips/conf/MALTA"

#ident 		"INSTALL_MALTA-$Revision: 1.1.2.2 $"

# Enable the hooks used for initializing the root memory-disk.
#     The ramdisk size must be kept in sync manually with the size of
#     the `ramdisk' image (which is built in distrib/evbmips/ramdisk/ramdisk).
pseudo-device	md				# memory disk device
options 	MEMORY_DISK_HOOKS
options 	MEMORY_DISK_IS_ROOT		# force root on memory disk
options 	MEMORY_DISK_SERVER=0		# no userspace memory disk
options 	MEMORY_DISK_ROOT_SIZE=12288	# size of memory disk, in blocks

makeoptions	NEED_MDSETIMAGE="yes"
