April 2014, Joel Porquet

This platform is known for being able to run Linux.

----
Pre-requisites:

* A working version of SoCLib
    - the command `soclib-cc --getpath` should return where SoCLib is installed
* A working version of TSAR
    - TSAR directory should be properly added to SoCLib's configuration: either
      globally, or through the `soclib.conf` file present in this directory (in
      which case, the environment variable `TSARDIR` should be defined to point
      on TSAR directory)


----
Targets of the Makefile:

* clean: clean the compilation files
* all (or none): compile the simulation system
* run_tsar_boot: runs the simulation system using a boot loader (in this case,
  you want to use a blockdevice image that contains the kernel: see `DSK`
  option below)
* run_dummy_boot: runs the simulation system using directly Linux instead of a
  boot loader (i.e. Linux is already loaded in RAM before execution).


----
Options for running:

These options apply when using either `run_tsar_boot` or `run_dummy_boot`
targets. Example: `make run_dummy_boot GDB=1 VMLINUX=../vmlinux DSK=dsk.img`

* GDB=1|[FXSCTZW]: options to the GDB server (1 means FCX which is a good
  default)
* NCPUS=[1-4]: number of processors
* DSK=[pathname]: path to a filesystem to use with the BlockDevice component
  (also implies creating a system with such a component, other the component is
  deactivated)
* TRACE=[number]: enables tracing the simulation starting from a certain cycle
* NCYCLES=[number]: runs the simulation for a certain number of cycles

    Only for run_dummy_boot:
    * VMLINUX=[pathname]: path to Linux `vmlinux` image


----
Using GDB server:

A file named `.gdbinit` contains a few macros that can be useful for debugging
Linux when using the GDB server.

* connect: connect to the GDB server that runs within the simulation
* dmesg: print the content of the kernel message buffer
* thread_info: print the thread_info structure of the current task
* task_struct: print the task_struct structure of the current task
* active_mm: print the active_mm structure of the current task
* pgd: print the content of the page table of the current task
* ps: print the list of running tasks

